

**New Balaji fire**

**and safety services**

Email : [balajifiresafety6@gmail.com](mailto:balajifiresafety6@gmail.com) Contact: 9326318479

Quotation

To :- -------------------- Date:-22/01/2025



SUB: QUOTATION FOR FIRE SAFETY FITTINGS

|  |  |  |  |
| --- | --- | --- | --- |
| **Sr. No** | **Work Description** | **Unit** | **Rate** |
| 1 | Erection, testing and commissioning of M.S/G.I Welded Joint Heavy grade Pipes with including of suitable types of M. S. supports, Anchor fastener, bullet fastener, thread rod, G. i. U &Hi-tech Clamp, Heavy grade Seamless fittings such as type of Reducers, Tees, elbows, flanges, & Forged type coupling, Socket elbow, With Two Coat Zinc Oxide & Two Coat of Red Paint, Including of Cutting, Drilling,Welding,Hanging, Loading, Unloading & Shifting etc. |  |  |
| *a* | 25 mm dia | per -mtr | 110 |
| *b* | 32 mm dia | per -mtr | 135 |
| *c* | 40 mm dia | per -mtr | 165 |
| *d* | 50 mm dia | per -mtr | 220 |
| *e* | 65 mm dia | per -mtr | 275 |
| *f* | 80 mm dia | per -mtr | 330 |
| *g* | 100 mm dia | per -mtr | 440 |
| *h* | 150 mm dia | per -mtr | 660 |
| *H.1* | Low zone Hydrant/Sprinkler raiser | per -mtr | 600 |
| *H.2* | High raise Hydrant /Sprinkler raiser | per -mtr | 660 |
| 2 | Erection, testing, and commissioning of M.S./G.I. welded joint heavy-grade pipes, butterfly valves with ball valves, drain line valves, flow switches, sight glass valves, and complete set, including suitable types of G.I. supports, anchor fasteners, bullet fasteners, threaded rods, G.I. U & Hi-Tech clamps, heavy-grade seamless fittings such as reducers, tees, elbows, flanges, and forged-type couplings, socket elbows with two coats of zinc oxide and two coats of red paint. This includes cutting, drilling, welding, hanging, loading, unloading, shifting, etc.Note : Price is including of Sprinkler Raiser tapping point to Sprinkler point.  **Note:** Price includes the sprinkler raiser tapping point to the sprinkler point. |  |  |
| a | Ground floor to 21th floor | per Point | 850 |
| b | 21th floor to upper floor | per Point | 950 |
| 3 | Installing, testing and commissioning of butterfly valves/ Sluice Valve/NRV/Foot Valve / Strainer etc. | per -mtr |  |
| a | 25 mm dia | per -mtr | 110 |
| b | 32 mm dia | per -mtr | 135 |
| c | 40 mm dia | per -mtr | 165 |
| *d* | 50 mm dia | per -mtr | 220 |
| *e* | 65 mm dia | per -mtr | 275 |
| *f* | 80 mm dia | per -mtr | 300 |
| *g* | 100 mm dia | per -mtr | 400 |
| a | 150 mm dia | per -mtr | 600 |
| 4 | Erection and fixing of MS Structure support with painting | Per-kg | 20 |
| 5 | Installing, testing and commissioning of Ball valve /Gate valve with fitting of screwed and complete set |  |  |
| *a* | 25 mm dia | per Nos | 100 |
| 6 | Installing, testing and commissioning of pressure gauges with middle pipe /middle cock with complete set | per Nos | 100 |
| 7 | Installing, testing and commissioning of Gun mettel Air release Valve with isolation valve with complete set. | per Nos | 100 |
| 8 | Installing, testing and commissioning of Sprinkler with Rosser Plate complete Set. |  |  |
| *a* | Pendent /Side wall/ Upright / Concealed / Drencher Nozzel / MVWS Nozzel / HVWS Nozzel / Sprinkler | per Nos | 50 |
| 9 | Installing, testing and commissioning of Flexodroup with Rosser plate complete Set 500 mm/1000 mm/1500 mm /2000 mm | per Nos | 250 |
| 10 | Installing, testing and commissioning of Hydrant Valve with Complete Set. |  |  |
| *a* | Singal Head Hydrant Valve | per Nos | 200 |
| *b* | Double Head Hydrant Valve | per Nos | 300 |
| 11 | Installing, testing and commissioning of Hose Box |  |  |
| *a* | Singal/Double door | per Nos | 200 |
| 12 | Installing, testing and commissioning of Hose Pipe | per Nos | 70 |
| 13 | Installing, testing and commissioning of Short branch pipe | per Nos | 50 |
| 14 | Installing, testing and commissioning of Hose reel drum of swining type with hose reel with Ball valve and shut off nozzel complete set | per Nos | 500 |
| 15 | Installing, testing and commissioning of Four way fire brigade Inlet and Outlet Breeching Complete Set. | per Nos | 400 |
| 16 | Installing, testing and commissioning of Deluge valves / Alarm Gong valve with complete Set. | per Nos | 2000 |
| 17 | Barden Type Wrapping and Coating With Black Japan |  |  |
| *a* | 80 mm/ 100mm / 150mm | per mtr | 15 |
| 18 | IWL Wrapping and Coating with Hot process |  |  |
| *a* | 80 mm/ 100mm / 150mm / 200 mm | per dia | 40 |
| 19 | Fixing of fire Extinguishers with mount brackets. |  |  |
| *a* | 4 Kg, 9 Kg , 6 Kg | per Nos | 70 |
| 20 | Fixing of fire bucket stand with with sand filling. | per Nos | 70 |
| 21 | Fixing of fire buckets stand with stand filling | per Nos | 100 |
| 22 | Installing, testing and commissioning of Pump room |  | \* |

**Terms & Conditions.**

1. Work order required to start the work.
2. 30%\* payment Advance before starting the work.
3. 55% payment required during work in progress.
4. 15% payment required after testing & finishing the work
5. All the additional Work will get chargeable.

Note: *In-case of any Concern feel free to reach on given contact details*

*All the (\* , TBD) can discuss on call and make a final price.*

**Proprietor .**

**Shailesh Rai**

